|  |  |
| --- | --- |
| FM Control Center | 1. **Receives** report of a lab building ventilation shutdown. |
|  | 1. **Notifies** appropriate shop for needed repairs. |
|  |  |
| FM Shop doing repairs | 1. **Requests** information on status of indoor air quality. 2. **Calls** EHS to determine need for respirator use and recommendations for repair personnel. 3. **Provides** an ETA on repairs to EHS personnel (see PRO-U5950.01F Entering A Building During Ventilation Shutdown With Hazardous Materials). 4. **Informs** EHS personnel when repairs complete. |